{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["故障日志"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"故障日志","index":0,"n_rows":193,"n_cols":12,"rows_kept":193,"cut":false,"hidden":false,"merged":[]}
["设备分类名称","设备分类编码","分类层级1","分类层级2","分类层级3","分类层级4","事件名称","事件ID","描述","标签","PLC地址","工位"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1000]_系统_HMI急停触发故障","A40000","AL[1000]_系统_HMI急停触发故障","故障类型：故障fault","fault_codes[0].0"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1001]_系统_急停1触发-前故障","A40001","AL[1001]_系统_急停1触发-前故障","故障类型：故障fault","fault_codes[0].1"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1002]_系统_急停2触发-后故障","A40002","AL[1002]_系统_急停2触发-后故障","故障类型：故障fault","fault_codes[0].2"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1003]_系统_机器人堵转故障","A40003","AL[1003]_系统_机器人堵转故障","故障类型：故障fault","fault_codes[0].3"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1004]_系统_XX故障","A40004","AL[1004]_系统_XX故障","故障类型：故障fault","fault_codes[0].4"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1005]_系统_XX故障","A40005","AL[1005]_系统_XX故障","故障类型：故障fault","fault_codes[0].5"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1006]_系统_XX故障","A40006","AL[1006]_系统_XX故障","故障类型：故障fault","fault_codes[0].6"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1007]_系统_XX故障","A40007","AL[1007]_系统_XX故障","故障类型：故障fault","fault_codes[0].7"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1008]_系统_XX故障","A40008","AL[1008]_系统_XX故障","故障类型：故障fault","fault_codes[0].8"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1009]_系统_XX故障","A40009","AL[1009]_系统_XX故障","故障类型：故障fault","fault_codes[0].9"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1010]_系统_XX故障","A40010","AL[1010]_系统_XX故障","故障类型：故障fault","fault_codes[0].10"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1011]_系统_XX故障","A40011","AL[1011]_系统_XX故障","故障类型：故障fault","fault_codes[0].11"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1012]_系统_XX故障","A40012","AL[1012]_系统_XX故障","故障类型：故障fault","fault_codes[0].12"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1013]_系统_XX故障","A40013","AL[1013]_系统_XX故障","故障类型：故障fault","fault_codes[0].13"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1014]_系统_XX故障","A40014","AL[1014]_系统_XX故障","故障类型：故障fault","fault_codes[0].14"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1015]_系统_XX故障","A40015","AL[1015]_系统_XX故障","故障类型：故障fault","fault_codes[0].15"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1016]_系统_XX故障","A40016","AL[1016]_系统_XX故障","故障类型：故障fault","fault_codes[0].16"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1017]_系统_XX故障","A40017","AL[1017]_系统_XX故障","故障类型：故障fault","fault_codes[0].17"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1018]_系统_XX故障","A40018","AL[1018]_系统_XX故障","故障类型：故障fault","fault_codes[0].18"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1019]_系统_XX故障","A40019","AL[1019]_系统_XX故障","故障类型：故障fault","fault_codes[0].19"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1020]_系统_XX故障","A40020","AL[1020]_系统_XX故障","故障类型：故障fault","fault_codes[0].20"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1021]_系统_XX故障","A40021","AL[1021]_系统_XX故障","故障类型：故障fault","fault_codes[0].21"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1022]_系统_XX故障","A40022","AL[1022]_系统_XX故障","故障类型：故障fault","fault_codes[0].22"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1023]_系统_XX故障","A40023","AL[1023]_系统_XX故障","故障类型：故障fault","fault_codes[0].23"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1024]_系统_XX故障","A40024","AL[1024]_系统_XX故障","故障类型：故障fault","fault_codes[0].24"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1025]_系统_XX故障","A40025","AL[1025]_系统_XX故障","故障类型：故障fault","fault_codes[0].25"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1026]_系统_XX故障","A40026","AL[1026]_系统_XX故障","故障类型：故障fault","fault_codes[0].26"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1027]_系统_XX故障","A40027","AL[1027]_系统_XX故障","故障类型：故障fault","fault_codes[0].27"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1028]_系统_XX故障","A40028","AL[1028]_系统_XX故障","故障类型：故障fault","fault_codes[0].28"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1029]_系统_XX故障","A40029","AL[1029]_系统_XX故障","故障类型：故障fault","fault_codes[0].29"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1030]_系统_XX故障","A40030","AL[1030]_系统_XX故障","故障类型：故障fault","fault_codes[0].30"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1031]_系统_XX故障","A40031","AL[1031]_系统_XX故障","故障类型：故障fault","fault_codes[0].31"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[0]_机器人_初始化超时警报","B40001","AL[0]_机器人_初始化超时警报","故障类型：警报alarm","fault_codes[1].0"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[1]_机器人_运行超时警报","B40002","AL[1]_机器人_运行超时警报","故障类型：警报alarm","fault_codes[1].1"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[2]_机器人_气缸上警报","B40003","AL[2]_机器人_气缸上警报","故障类型：警报alarm","fault_codes[1].2"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[3]_机器人_气缸下警报","B40004","AL[3]_机器人_气缸下警报","故障类型：警报alarm","fault_codes[1].3"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[4]_机器人_防掉气缸伸出警报","B40005","AL[4]_机器人_防掉气缸伸出警报","故障类型：警报alarm","fault_codes[1].4"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[5]_机器人_防掉气缸缩回警报","B40006","AL[5]_机器人_防掉气缸缩回警报","故障类型：警报alarm","fault_codes[1].5"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[6]_机器人_真空1警报","B40007","AL[6]_机器人_真空1警报","故障类型：警报alarm","fault_codes[1].6"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[7]_机器人_真空2警报","B40008","AL[7]_机器人_真空2警报","故障类型：警报alarm","fault_codes[1].7"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[8]_机器人_XX警报","B40009","AL[8]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].8"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[9]_机器人_XX警报","B40010","AL[9]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].9"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[10]_机器人_XX警报","B40011","AL[10]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].10"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[11]_机器人_XX警报","B40012","AL[11]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].11"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[12]_机器人_XX警报","B40013","AL[12]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].12"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[13]_机器人_XX警报","B40014","AL[13]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].13"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[14]_机器人_XX警报","B40015","AL[14]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].14"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[15]_机器人_XX警报","B40016","AL[15]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].15"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[16]_机器人_XX警报","B40017","AL[16]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].16"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[17]_机器人_XX警报","B40018","AL[17]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].17"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[18]_机器人_XX警报","B40019","AL[18]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].18"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[19]_机器人_XX警报","B40020","AL[19]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].19"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[20]_机器人_XX警报","B40021","AL[20]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].20"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[21]_机器人_XX警报","B40022","AL[21]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].21"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[22]_机器人_XX警报","B40023","AL[22]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].22"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[23]_机器人_XX警报","B40024","AL[23]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].23"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[24]_机器人_XX警报","B40025","AL[24]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].24"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[25]_机器人_XX警报","B40026","AL[25]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].25"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[26]_机器人_XX警报","B40027","AL[26]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].26"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[27]_机器人_XX警报","B40028","AL[27]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].27"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[28]_机器人_XX警报","B40029","AL[28]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].28"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[29]_机器人_XX警报","B40030","AL[29]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].29"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[30]_机器人_XX警报","B40031","AL[30]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].30"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[31]_机器人_XX警报","B40032","AL[31]_机器人_XX警报","故障类型：警报alarm","fault_codes[1].31"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[32]_作业线_初始化超时警报","B40033","AL[32]_作业线_初始化超时警报","故障类型：警报alarm","fault_codes[2].0"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[33]_作业线_运行超时警报","B40034","AL[33]_作业线_运行超时警报","故障类型：警报alarm","fault_codes[2].1"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[34]_作业线_载具到位超时警报","B40035","AL[34]_作业线_载具到位超时警报","故障类型：警报alarm","fault_codes[2].2"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[35]_作业线_载具离开超时警报","B40036","AL[35]_作业线_载具离开超时警报","故障类型：警报alarm","fault_codes[2].3"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[36]_作业线_顶升上警报","B40037","AL[36]_作业线_顶升上警报","故障类型：警报alarm","fault_codes[2].4"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[37]_作业线_顶升下警报","B40038","AL[37]_作业线_顶升下警报","故障类型：警报alarm","fault_codes[2].5"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[38]_作业线_NG台警报","B40039","AL[38]_作业线_NG台警报","故障类型：警报alarm","fault_codes[2].6"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[39]_作业线_XX警报","B40040","AL[39]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].7"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[40]_作业线_XX警报","B40041","AL[40]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].8"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[41]_作业线_XX警报","B40042","AL[41]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].9"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[42]_作业线_XX警报","B40043","AL[42]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].10"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[43]_作业线_XX警报","B40044","AL[43]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].11"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[44]_作业线_XX警报","B40045","AL[44]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].12"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[45]_作业线_XX警报","B40046","AL[45]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].13"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[46]_作业线_XX警报","B40047","AL[46]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].14"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[47]_作业线_XX警报","B40048","AL[47]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].15"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[48]_作业线_XX警报","B40049","AL[48]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].16"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[49]_作业线_XX警报","B40050","AL[49]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].17"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[50]_作业线_XX警报","B40051","AL[50]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].18"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[51]_作业线_XX警报","B40052","AL[51]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].19"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[52]_作业线_XX警报","B40053","AL[52]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].20"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[53]_作业线_XX警报","B40054","AL[53]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].21"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[54]_作业线_XX警报","B40055","AL[54]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].22"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[55]_作业线_XX警报","B40056","AL[55]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].23"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[56]_作业线_XX警报","B40057","AL[56]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].24"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[57]_作业线_XX警报","B40058","AL[57]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].25"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[58]_作业线_XX警报","B40059","AL[58]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].26"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[59]_作业线_XX警报","B40060","AL[59]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].27"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[60]_作业线_XX警报","B40061","AL[60]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].28"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[61]_作业线_XX警报","B40062","AL[61]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].29"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[62]_作业线_XX警报","B40063","AL[62]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].30"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[63]_作业线_XX警报","B40064","AL[63]_作业线_XX警报","故障类型：警报alarm","fault_codes[2].31"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[64]_翻转机构_初始化超时警报","B40065","AL[64]_翻转机构_初始化超时警报","故障类型：警报alarm","fault_codes[3].0"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[65]_翻转机构_运行超时警报","B40066","AL[65]_翻转机构_运行超时警报","故障类型：警报alarm","fault_codes[3].1"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[66]_翻转机构_轴错误警报","B40067","AL[66]_翻转机构_轴错误警报","故障类型：警报alarm","fault_codes[3].2"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[67]_翻转机构_顶升上警报","B40068","AL[67]_翻转机构_顶升上警报","故障类型：警报alarm","fault_codes[3].3"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[68]_翻转机构_顶升下警报","B40069","AL[68]_翻转机构_顶升下警报","故障类型：警报alarm","fault_codes[3].4"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[69]_翻转机构_真空1警报","B40070","AL[69]_翻转机构_真空1警报","故障类型：警报alarm","fault_codes[3].5"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[70]_翻转机构_真空2警报","B40071","AL[70]_翻转机构_真空2警报","故障类型：警报alarm","fault_codes[3].6"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[71]_翻转机构_XX警报","B40072","AL[71]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].7"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[72]_翻转机构_XX警报","B40073","AL[72]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].8"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[73]_翻转机构_XX警报","B40074","AL[73]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].9"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[74]_翻转机构_XX警报","B40075","AL[74]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].10"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[75]_翻转机构_XX警报","B40076","AL[75]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].11"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[76]_翻转机构_XX警报","B40077","AL[76]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].12"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[77]_翻转机构_XX警报","B40078","AL[77]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].13"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[78]_翻转机构_XX警报","B40079","AL[78]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].14"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[79]_翻转机构_XX警报","B40080","AL[79]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].15"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[80]_翻转机构_XX警报","B40081","AL[80]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].16"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[81]_翻转机构_XX警报","B40082","AL[81]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].17"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[82]_翻转机构_XX警报","B40083","AL[82]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].18"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[83]_翻转机构_XX警报","B40084","AL[83]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].19"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[84]_翻转机构_XX警报","B40085","AL[84]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].20"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[85]_翻转机构_XX警报","B40086","AL[85]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].21"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[86]_翻转机构_XX警报","B40087","AL[86]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].22"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[87]_翻转机构_XX警报","B40088","AL[87]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].23"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[88]_翻转机构_XX警报","B40089","AL[88]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].24"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[89]_翻转机构_XX警报","B40090","AL[89]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].25"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[90]_翻转机构_XX警报","B40091","AL[90]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].26"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[91]_翻转机构_XX警报","B40092","AL[91]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].27"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[92]_翻转机构_XX警报","B40093","AL[92]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].28"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[93]_翻转机构_XX警报","B40094","AL[93]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].29"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[94]_翻转机构_XX警报","B40095","AL[94]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].30"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[95]_翻转机构_XX警报","B40096","AL[95]_翻转机构_XX警报","故障类型：警报alarm","fault_codes[3].31"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[96]_回流线_初始化超时警报","B40097","AL[96]_回流线_初始化超时警报","故障类型：警报alarm","fault_codes[4].0"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[97]_回流线_运行超时警报","B40098","AL[97]_回流线_运行超时警报","故障类型：警报alarm","fault_codes[4].1"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[98]_回流线_XX警报","B40099","AL[98]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].2"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[99]_回流线_XX警报","B40100","AL[99]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].3"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[100]_回流线_XX警报","B40101","AL[100]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].4"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[101]_回流线_XX警报","B40102","AL[101]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].5"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[102]_回流线_XX警报","B40103","AL[102]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].6"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[103]_回流线_XX警报","B40104","AL[103]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].7"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[104]_回流线_XX警报","B40105","AL[104]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].8"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[105]_回流线_XX警报","B40106","AL[105]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].9"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[106]_回流线_XX警报","B40107","AL[106]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].10"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[107]_回流线_XX警报","B40108","AL[107]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].11"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[108]_回流线_XX警报","B40109","AL[108]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].12"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[109]_回流线_XX警报","B40110","AL[109]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].13"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[110]_回流线_XX警报","B40111","AL[110]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].14"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[111]_回流线_XX警报","B40112","AL[111]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].15"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[112]_回流线_XX警报","B40113","AL[112]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].16"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[113]_回流线_XX警报","B40114","AL[113]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].17"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[114]_回流线_XX警报","B40115","AL[114]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].18"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[115]_回流线_XX警报","B40116","AL[115]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].19"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[116]_回流线_XX警报","B40117","AL[116]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].20"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[117]_回流线_XX警报","B40118","AL[117]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].21"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[118]_回流线_XX警报","B40119","AL[118]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].22"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[119]_回流线_XX警报","B40120","AL[119]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].23"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[120]_回流线_XX警报","B40121","AL[120]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].24"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[121]_回流线_XX警报","B40122","AL[121]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].25"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[122]_回流线_XX警报","B40123","AL[122]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].26"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[123]_回流线_XX警报","B40124","AL[123]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].27"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[124]_回流线_XX警报","B40125","AL[124]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].28"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[125]_回流线_XX警报","B40126","AL[125]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].29"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[126]_回流线_XX警报","B40127","AL[126]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].30"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[127]_回流线_XX警报","B40128","AL[127]_回流线_XX警报","故障类型：警报alarm","fault_codes[4].31"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[128]_系统_总气源压力警报","B40129","AL[128]_系统_总气源压力警报","故障类型：警报alarm","fault_codes[5].0"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[129]_系统_后右下安全门警报","B40130","AL[129]_系统_后右下安全门警报","故障类型：警报alarm","fault_codes[5].1"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[130]_系统_后左下安全门警报","B40131","AL[130]_系统_后左下安全门警报","故障类型：警报alarm","fault_codes[5].2"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[131]_系统_前右安全门警报","B40132","AL[131]_系统_前右安全门警报","故障类型：警报alarm","fault_codes[5].3"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[132]_系统_后左安全门警报","B40133","AL[132]_系统_后左安全门警报","故障类型：警报alarm","fault_codes[5].4"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[133]_系统_前左安全门警报","B40134","AL[133]_系统_前左安全门警报","故障类型：警报alarm","fault_codes[5].5"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[134]_系统_前左下安全门警报","B40135","AL[134]_系统_前左下安全门警报","故障类型：警报alarm","fault_codes[5].6"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[135]_系统_后右安全门警报","B40136","AL[135]_系统_后右安全门警报","故障类型：警报alarm","fault_codes[5].7"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[136]_系统_前右下安全门警报","B40137","AL[136]_系统_前右下安全门警报","故障类型：警报alarm","fault_codes[5].8"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[137]_系统_光栅警报","B40138","AL[137]_系统_光栅警报","故障类型：警报alarm","fault_codes[5].9"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[138]_系统_XX警报","B40139","AL[138]_系统_XX警报","故障类型：警报alarm","fault_codes[5].10"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[139]_系统_XX警报","B40140","AL[139]_系统_XX警报","故障类型：警报alarm","fault_codes[5].11"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[140]_系统_XX警报","B40141","AL[140]_系统_XX警报","故障类型：警报alarm","fault_codes[5].12"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[141]_系统_XX警报","B40142","AL[141]_系统_XX警报","故障类型：警报alarm","fault_codes[5].13"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[142]_系统_XX警报","B40143","AL[142]_系统_XX警报","故障类型：警报alarm","fault_codes[5].14"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[143]_系统_XX警报","B40144","AL[143]_系统_XX警报","故障类型：警报alarm","fault_codes[5].15"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[144]_系统_XX警报","B40145","AL[144]_系统_XX警报","故障类型：警报alarm","fault_codes[5].16"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[145]_系统_XX警报","B40146","AL[145]_系统_XX警报","故障类型：警报alarm","fault_codes[5].17"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[146]_系统_XX警报","B40147","AL[146]_系统_XX警报","故障类型：警报alarm","fault_codes[5].18"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[147]_系统_XX警报","B40148","AL[147]_系统_XX警报","故障类型：警报alarm","fault_codes[5].19"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[148]_系统_XX警报","B40149","AL[148]_系统_XX警报","故障类型：警报alarm","fault_codes[5].20"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[149]_系统_XX警报","B40150","AL[149]_系统_XX警报","故障类型：警报alarm","fault_codes[5].21"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[150]_系统_XX警报","B40151","AL[150]_系统_XX警报","故障类型：警报alarm","fault_codes[5].22"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[151]_系统_XX警报","B40152","AL[151]_系统_XX警报","故障类型：警报alarm","fault_codes[5].23"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[152]_系统_XX警报","B40153","AL[152]_系统_XX警报","故障类型：警报alarm","fault_codes[5].24"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[153]_系统_XX警报","B40154","AL[153]_系统_XX警报","故障类型：警报alarm","fault_codes[5].25"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[154]_系统_XX警报","B40155","AL[154]_系统_XX警报","故障类型：警报alarm","fault_codes[5].26"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[155]_系统_XX警报","B40156","AL[155]_系统_XX警报","故障类型：警报alarm","fault_codes[5].27"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[156]_系统_XX警报","B40157","AL[156]_系统_XX警报","故障类型：警报alarm","fault_codes[5].28"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[157]_系统_XX警报","B40158","AL[157]_系统_XX警报","故障类型：警报alarm","fault_codes[5].29"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[158]_系统_XX警报","B40159","AL[158]_系统_XX警报","故障类型：警报alarm","fault_codes[5].30"]
["组上盖板","C-PFA-CPPCT-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","整机模块\n overall_module","AL[159]_系统_XX警报","B40160","AL[159]_系统_XX警报","故障类型：警报alarm","fault_codes[5].31"]