{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["故障日志"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"故障日志","index":0,"n_rows":321,"n_cols":12,"rows_kept":321,"cut":false,"hidden":false,"merged":[]}
["设备分类名称","设备分类编码","分类层级1","分类层级2","分类层级3","分类层级4","事件名称","事件ID","描述","标签","PLC地址","工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1000]_系统_HMI急停触发故障","A40000","AL[1000]_系统_HMI急停触发故障","故障类型：故障fault","fault_codes[0].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1001]_系统_急停1触发-前故障","A40001","AL[1001]_系统_急停1触发-前故障","故障类型：故障fault","fault_codes[0].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1002]_系统_急停2触发-后故障","A40002","AL[1002]_系统_急停2触发-后故障","故障类型：故障fault","fault_codes[0].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1003]_系统_急停3触发故障","A40003","AL[1003]_系统_急停3触发故障","故障类型：故障fault","fault_codes[0].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1004]_系统_气源检测警报警报","A40004","AL[1004]_系统_气源检测警报警报","故障类型：故障fault","fault_codes[0].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1005]_系统_XX警报","A40005","AL[1005]_系统_XX警报","故障类型：故障fault","fault_codes[0].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1006]_系统_XX警报","A40006","AL[1006]_系统_XX警报","故障类型：故障fault","fault_codes[0].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1007]_系统_关门检测1NO-后上左侧警报","A40007","AL[1007]_系统_关门检测1NO-后上左侧警报","故障类型：故障fault","fault_codes[0].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1008]_系统_关门检测2NO-后上右侧警报","A40008","AL[1008]_系统_关门检测2NO-后上右侧警报","故障类型：故障fault","fault_codes[0].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1009]_系统_关门检测3NO-后下左侧警报","A40009","AL[1009]_系统_关门检测3NO-后下左侧警报","故障类型：故障fault","fault_codes[0].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1010]_系统_关门检测4NO-后下右侧警报","A40010","AL[1010]_系统_关门检测4NO-后下右侧警报","故障类型：故障fault","fault_codes[0].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1011]_系统_关门检测5NO-前上左侧警报","A40011","AL[1011]_系统_关门检测5NO-前上左侧警报","故障类型：故障fault","fault_codes[0].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1012]_系统_关门检测6NO-前上右侧警报","A40012","AL[1012]_系统_关门检测6NO-前上右侧警报","故障类型：故障fault","fault_codes[0].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1013]_系统_关门检测7NO-前下左侧警报","A40013","AL[1013]_系统_关门检测7NO-前下左侧警报","故障类型：故障fault","fault_codes[0].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1014]_系统_关门检测8NO-前下右侧警报","A40014","AL[1014]_系统_关门检测8NO-前下右侧警报","故障类型：故障fault","fault_codes[0].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1015]_系统_XX警报","A40015","AL[1015]_系统_XX警报","故障类型：故障fault","fault_codes[0].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1016]_系统_XX警报","A40016","AL[1016]_系统_XX警报","故障类型：故障fault","fault_codes[0].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1017]_系统_XX警报","A40017","AL[1017]_系统_XX警报","故障类型：故障fault","fault_codes[0].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1018]_系统_XX警报","A40018","AL[1018]_系统_XX警报","故障类型：故障fault","fault_codes[0].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1019]_系统_XX警报","A40019","AL[1019]_系统_XX警报","故障类型：故障fault","fault_codes[0].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1020]_系统_XX警报","A40020","AL[1020]_系统_XX警报","故障类型：故障fault","fault_codes[0].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1021]_系统_XX故障","A40021","AL[1021]_系统_XX故障","故障类型：故障fault","fault_codes[0].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1022]_系统_XX故障","A40022","AL[1022]_系统_XX故障","故障类型：故障fault","fault_codes[0].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1023]_系统_XX故障","A40023","AL[1023]_系统_XX故障","故障类型：故障fault","fault_codes[0].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1024]_系统_XX故障","A40024","AL[1024]_系统_XX故障","故障类型：故障fault","fault_codes[0].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1025]_系统_XX故障","A40025","AL[1025]_系统_XX故障","故障类型：故障fault","fault_codes[0].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1026]_系统_XX故障","A40026","AL[1026]_系统_XX故障","故障类型：故障fault","fault_codes[0].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1027]_系统_XX故障","A40027","AL[1027]_系统_XX故障","故障类型：故障fault","fault_codes[0].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1028]_系统_XX故障","A40028","AL[1028]_系统_XX故障","故障类型：故障fault","fault_codes[0].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1029]_系统_XX故障","A40029","AL[1029]_系统_XX故障","故障类型：故障fault","fault_codes[0].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1030]_系统_XX故障","A40030","AL[1030]_系统_XX故障","故障类型：故障fault","fault_codes[0].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","故障\n fault","整机模块\n overall_module","AL[1031]_系统_XX故障","A40031","AL[1031]_系统_XX故障","故障类型：故障fault","fault_codes[0].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[0]_三轴定位拍照机构_运行超时警报","B40001","AL[0]_三轴定位拍照机构_运行超时警报","故障类型：警报alarm","fault_codes[1].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[1]_三轴定位拍照机构_三轴初始化超时警报","B40002","AL[1]_三轴定位拍照机构_三轴初始化超时警报","故障类型：警报alarm","fault_codes[1].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[2]_三轴定位拍照机构_2D相机警报","B40003","AL[2]_三轴定位拍照机构_2D相机警报","故障类型：警报alarm","fault_codes[1].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[3]_三轴定位拍照机构_3D相机警报","B40004","AL[3]_三轴定位拍照机构_3D相机警报","故障类型：警报alarm","fault_codes[1].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[4]_三轴定位拍照机构_初始化OK环境异常，X轴伺服位置已偏离原点警报","B40005","AL[4]_三轴定位拍照机构_初始化OK环境异常，X轴伺服位置已偏离原点警报","故障类型：警报alarm","fault_codes[1].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[5]_三轴定位拍照机构_初始化OK环境异常，Y轴伺服位置已偏离原点警报","B40006","AL[5]_三轴定位拍照机构_初始化OK环境异常，Y轴伺服位置已偏离原点警报","故障类型：警报alarm","fault_codes[1].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[6]_三轴定位拍照机构_初始化OK环境异常，Z轴伺服位置已偏离原点警报","B40007","AL[6]_三轴定位拍照机构_初始化OK环境异常，Z轴伺服位置已偏离原点警报","故障类型：警报alarm","fault_codes[1].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[7]_三轴定位拍照机构_初始化OK环境异常，备用警报","B40008","AL[7]_三轴定位拍照机构_初始化OK环境异常，备用警报","故障类型：警报alarm","fault_codes[1].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[8]_三轴定位拍照机构_XX警报","B40009","AL[8]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[9]_三轴定位拍照机构_XX警报","B40010","AL[9]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[10]_三轴定位拍照机构_X轴警报","B40011","AL[10]_三轴定位拍照机构_X轴警报","故障类型：警报alarm","fault_codes[1].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[11]_三轴定位拍照机构_X轴到达正限位位置警报","B40012","AL[11]_三轴定位拍照机构_X轴到达正限位位置警报","故障类型：警报alarm","fault_codes[1].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[12]_三轴定位拍照机构_X轴到达负限位位置警报","B40013","AL[12]_三轴定位拍照机构_X轴到达负限位位置警报","故障类型：警报alarm","fault_codes[1].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[13]_三轴定位拍照机构_Y轴警报","B40014","AL[13]_三轴定位拍照机构_Y轴警报","故障类型：警报alarm","fault_codes[1].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[14]_三轴定位拍照机构_Y轴到达正限位位置警报","B40015","AL[14]_三轴定位拍照机构_Y轴到达正限位位置警报","故障类型：警报alarm","fault_codes[1].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[15]_三轴定位拍照机构_Y轴到达负限位位置警报","B40016","AL[15]_三轴定位拍照机构_Y轴到达负限位位置警报","故障类型：警报alarm","fault_codes[1].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[16]_三轴定位拍照机构_Z轴警报","B40017","AL[16]_三轴定位拍照机构_Z轴警报","故障类型：警报alarm","fault_codes[1].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[17]_三轴定位拍照机构_Z轴到达正限位位置警报","B40018","AL[17]_三轴定位拍照机构_Z轴到达正限位位置警报","故障类型：警报alarm","fault_codes[1].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[18]_三轴定位拍照机构_Z轴到达负限位位置警报","B40019","AL[18]_三轴定位拍照机构_Z轴到达负限位位置警报","故障类型：警报alarm","fault_codes[1].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[19]_三轴定位拍照机构_自动模式暂停环境异常，X轴位置距离停止位置发生偏移警报","B40020","AL[19]_三轴定位拍照机构_自动模式暂停环境异常，X轴位置距离停止位置发生偏移警报","故障类型：警报alarm","fault_codes[1].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[20]_三轴定位拍照机构_自动模式暂停环境异常，Y轴位置距离停止位置发生偏移警报","B40021","AL[20]_三轴定位拍照机构_自动模式暂停环境异常，Y轴位置距离停止位置发生偏移警报","故障类型：警报alarm","fault_codes[1].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[21]_三轴定位拍照机构_自动模式暂停环境异常，Z轴位置距离停止位置发生偏移警报","B40022","AL[21]_三轴定位拍照机构_自动模式暂停环境异常，Z轴位置距离停止位置发生偏移警报","故障类型：警报alarm","fault_codes[1].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[22]_三轴定位拍照机构_自动模式暂停环境异常，备用警报","B40023","AL[22]_三轴定位拍照机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[1].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[23]_三轴定位拍照机构_自动模式暂停环境异常，备用警报","B40024","AL[23]_三轴定位拍照机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[1].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[24]_三轴定位拍照机构_XX警报","B40025","AL[24]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[25]_三轴定位拍照机构_XX警报","B40026","AL[25]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[26]_三轴定位拍照机构_XX警报","B40027","AL[26]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[27]_三轴定位拍照机构_XX警报","B40028","AL[27]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[28]_三轴定位拍照机构_XX警报","B40029","AL[28]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[29]_三轴定位拍照机构_XX警报","B40030","AL[29]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[30]_三轴定位拍照机构_XX警报","B40031","AL[30]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[31]_三轴定位拍照机构_XX警报","B40032","AL[31]_三轴定位拍照机构_XX警报","故障类型：警报alarm","fault_codes[1].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[32]_作业线顶升机构_运行超时警报","B40033","AL[32]_作业线顶升机构_运行超时警报","故障类型：警报alarm","fault_codes[2].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[33]_作业线顶升机构_初始化超时警报","B40034","AL[33]_作业线顶升机构_初始化超时警报","故障类型：警报alarm","fault_codes[2].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[34]_作业线顶升机构_顶升气缸静点警报","B40035","AL[34]_作业线顶升机构_顶升气缸静点警报","故障类型：警报alarm","fault_codes[2].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[35]_作业线顶升机构_顶升气缸动点警报","B40036","AL[35]_作业线顶升机构_顶升气缸动点警报","故障类型：警报alarm","fault_codes[2].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[36]_作业线顶升机构_扫码枪警报","B40037","AL[36]_作业线顶升机构_扫码枪警报","故障类型：警报alarm","fault_codes[2].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[37]_作业线顶升机构_XX警报","B40038","AL[37]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[38]_作业线顶升机构_XX警报","B40039","AL[38]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[39]_作业线顶升机构_XX警报","B40040","AL[39]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[40]_作业线顶升机构_初始化OK环境异常，作业线顶升平台需要落下警报","B40041","AL[40]_作业线顶升机构_初始化OK环境异常，作业线顶升平台需要落下警报","故障类型：警报alarm","fault_codes[2].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[41]_作业线顶升机构_初始化OK环境异常，作业线阻挡需要升起警报","B40042","AL[41]_作业线顶升机构_初始化OK环境异常，作业线阻挡需要升起警报","故障类型：警报alarm","fault_codes[2].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[42]_作业线顶升机构_初始化OK环境异常，备用警报","B40043","AL[42]_作业线顶升机构_初始化OK环境异常，备用警报","故障类型：警报alarm","fault_codes[2].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[43]_作业线顶升机构_初始化OK环境异常，备用警报","B40044","AL[43]_作业线顶升机构_初始化OK环境异常，备用警报","故障类型：警报alarm","fault_codes[2].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[44]_作业线顶升机构_初始化OK环境异常，作业线电机需要停止警报","B40045","AL[44]_作业线顶升机构_初始化OK环境异常，作业线电机需要停止警报","故障类型：警报alarm","fault_codes[2].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[45]_作业线顶升机构_自动模式暂停环境异常，作业线输送线阻挡状态被改变警报","B40046","AL[45]_作业线顶升机构_自动模式暂停环境异常，作业线输送线阻挡状态被改变警报","故障类型：警报alarm","fault_codes[2].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[46]_作业线顶升机构_自动模式暂停环境异常，作业线输送线顶升气缸状态被改变警报","B40047","AL[46]_作业线顶升机构_自动模式暂停环境异常，作业线输送线顶升气缸状态被改变警报","故障类型：警报alarm","fault_codes[2].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[47]_作业线顶升机构_自动模式暂停环境异常，备用警报","B40048","AL[47]_作业线顶升机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[2].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[48]_作业线顶升机构_自动模式暂停环境异常，备用警报","B40049","AL[48]_作业线顶升机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[2].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[49]_作业线顶升机构_自动模式暂停环境异常，备用警报","B40050","AL[49]_作业线顶升机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[2].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[50]_作业线顶升机构_自动模式暂停环境异常，作业线电机状态被改变警报","B40051","AL[50]_作业线顶升机构_自动模式暂停环境异常，作业线电机状态被改变警报","故障类型：警报alarm","fault_codes[2].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[51]_作业线顶升机构_自动模式暂停环境异常，备用警报","B40052","AL[51]_作业线顶升机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[2].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[52]_作业线顶升机构_自动模式暂停环境异常，备用警报","B40053","AL[52]_作业线顶升机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[2].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[53]_作业线顶升机构_自动模式暂停环境异常，备用警报","B40054","AL[53]_作业线顶升机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[2].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[54]_作业线顶升机构_XX警报","B40055","AL[54]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[55]_作业线顶升机构_XX警报","B40056","AL[55]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[56]_作业线顶升机构_XX警报","B40057","AL[56]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[57]_作业线顶升机构_XX警报","B40058","AL[57]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[58]_作业线顶升机构_XX警报","B40059","AL[58]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[59]_作业线顶升机构_XX警报","B40060","AL[59]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[60]_作业线顶升机构_XX警报","B40061","AL[60]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[61]_作业线顶升机构_XX警报","B40062","AL[61]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[62]_作业线顶升机构_XX警报","B40063","AL[62]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[63]_作业线顶升机构_XX警报","B40064","AL[63]_作业线顶升机构_XX警报","故障类型：警报alarm","fault_codes[2].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[64]_回流机构_运行超时警报","B40065","AL[64]_回流机构_运行超时警报","故障类型：警报alarm","fault_codes[3].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[65]_回流机构_初始化超时警报","B40066","AL[65]_回流机构_初始化超时警报","故障类型：警报alarm","fault_codes[3].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[66]_回流机构_初始化OK环境异常，回流线电机需要停止警报","B40067","AL[66]_回流机构_初始化OK环境异常，回流线电机需要停止警报","故障类型：警报alarm","fault_codes[3].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[67]_回流机构_初始化OK环境异常，备用警报","B40068","AL[67]_回流机构_初始化OK环境异常，备用警报","故障类型：警报alarm","fault_codes[3].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[68]_回流机构_初始化OK环境异常，备用警报","B40069","AL[68]_回流机构_初始化OK环境异常，备用警报","故障类型：警报alarm","fault_codes[3].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[69]_回流机构_自动模式暂停环境异常，回流线电机状态被改变警报","B40070","AL[69]_回流机构_自动模式暂停环境异常，回流线电机状态被改变警报","故障类型：警报alarm","fault_codes[3].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[70]_回流机构_自动模式暂停环境异常，备用警报","B40071","AL[70]_回流机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[3].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[71]_回流机构_自动模式暂停环境异常，备用警报","B40072","AL[71]_回流机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[3].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[72]_回流机构_自动模式暂停环境异常，备用警报","B40073","AL[72]_回流机构_自动模式暂停环境异常，备用警报","故障类型：警报alarm","fault_codes[3].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[73]_回流机构_XX警报","B40074","AL[73]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[74]_回流机构_XX警报","B40075","AL[74]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[75]_回流机构_XX警报","B40076","AL[75]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[76]_回流机构_XX警报","B40077","AL[76]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[77]_回流机构_XX警报","B40078","AL[77]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[78]_回流机构_XX警报","B40079","AL[78]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[79]_回流机构_XX警报","B40080","AL[79]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[80]_回流机构_XX警报","B40081","AL[80]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[81]_回流机构_XX警报","B40082","AL[81]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[82]_回流机构_XX警报","B40083","AL[82]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[83]_回流机构_XX警报","B40084","AL[83]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[84]_回流机构_XX警报","B40085","AL[84]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[85]_回流机构_XX警报","B40086","AL[85]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[86]_回流机构_XX警报","B40087","AL[86]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[87]_回流机构_XX警报","B40088","AL[87]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[88]_回流机构_XX警报","B40089","AL[88]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[89]_回流机构_XX警报","B40090","AL[89]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[90]_回流机构_XX警报","B40091","AL[90]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[91]_回流机构_XX警报","B40092","AL[91]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[92]_回流机构_XX警报","B40093","AL[92]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[93]_回流机构_XX警报","B40094","AL[93]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[94]_回流机构_XX警报","B40095","AL[94]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n work_module","AL[95]_回流机构_XX警报","B40096","AL[95]_回流机构_XX警报","故障类型：警报alarm","fault_codes[3].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[96]_单元4_XX警报","B40097","AL[96]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[97]_单元4_XX警报","B40098","AL[97]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[98]_单元4_XX警报","B40099","AL[98]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[99]_单元4_XX警报","B40100","AL[99]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[100]_单元4_XX警报","B40101","AL[100]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[101]_单元4_XX警报","B40102","AL[101]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[102]_单元4_XX警报","B40103","AL[102]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[103]_单元4_XX警报","B40104","AL[103]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[104]_单元4_XX警报","B40105","AL[104]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[105]_单元4_XX警报","B40106","AL[105]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[106]_单元4_XX警报","B40107","AL[106]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[107]_单元4_XX警报","B40108","AL[107]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[108]_单元4_XX警报","B40109","AL[108]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[109]_单元4_XX警报","B40110","AL[109]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[110]_单元4_XX警报","B40111","AL[110]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[111]_单元4_XX警报","B40112","AL[111]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[112]_单元4_XX警报","B40113","AL[112]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[113]_单元4_XX警报","B40114","AL[113]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[114]_单元4_XX警报","B40115","AL[114]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[115]_单元4_XX警报","B40116","AL[115]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[116]_单元4_XX警报","B40117","AL[116]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[117]_单元4_XX警报","B40118","AL[117]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[118]_单元4_XX警报","B40119","AL[118]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[119]_单元4_XX警报","B40120","AL[119]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[120]_单元4_XX警报","B40121","AL[120]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[121]_单元4_XX警报","B40122","AL[121]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[122]_单元4_XX警报","B40123","AL[122]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[123]_单元4_XX警报","B40124","AL[123]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[124]_单元4_XX警报","B40125","AL[124]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[125]_单元4_XX警报","B40126","AL[125]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[126]_单元4_XX警报","B40127","AL[126]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[127]_单元4_XX警报","B40128","AL[127]_单元4_XX警报","故障类型：警报alarm","fault_codes[4].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[128]_单元5_XX警报","B40129","AL[128]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[129]_单元5_XX警报","B40130","AL[129]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[130]_单元5_XX警报","B40131","AL[130]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[131]_单元5_XX警报","B40132","AL[131]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[132]_单元5_XX警报","B40133","AL[132]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[133]_单元5_XX警报","B40134","AL[133]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[134]_单元5_XX警报","B40135","AL[134]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[135]_单元5_XX警报","B40136","AL[135]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[136]_单元5_XX警报","B40137","AL[136]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[137]_单元5_XX警报","B40138","AL[137]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[138]_单元5_XX警报","B40139","AL[138]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[139]_单元5_XX警报","B40140","AL[139]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[140]_单元5_XX警报","B40141","AL[140]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[141]_单元5_XX警报","B40142","AL[141]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[142]_单元5_XX警报","B40143","AL[142]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[143]_单元5_XX警报","B40144","AL[143]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[144]_单元5_XX警报","B40145","AL[144]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[145]_单元5_XX警报","B40146","AL[145]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[146]_单元5_XX警报","B40147","AL[146]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[147]_单元5_XX警报","B40148","AL[147]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[148]_单元5_XX警报","B40149","AL[148]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[149]_单元5_XX警报","B40150","AL[149]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[150]_单元5_XX警报","B40151","AL[150]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[151]_单元5_XX警报","B40152","AL[151]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[152]_单元5_XX警报","B40153","AL[152]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[153]_单元5_XX警报","B40154","AL[153]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[154]_单元5_XX警报","B40155","AL[154]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[155]_单元5_XX警报","B40156","AL[155]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[156]_单元5_XX警报","B40157","AL[156]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[157]_单元5_XX警报","B40158","AL[157]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[158]_单元5_XX警报","B40159","AL[158]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[159]_单元5_XX警报","B40160","AL[159]_单元5_XX警报","故障类型：警报alarm","fault_codes[5].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[160]_单元6_XX警报","B40161","AL[160]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[161]_单元6_XX警报","B40162","AL[161]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[162]_单元6_XX警报","B40163","AL[162]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[163]_单元6_XX警报","B40164","AL[163]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[164]_单元6_XX警报","B40165","AL[164]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[165]_单元6_XX警报","B40166","AL[165]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[166]_单元6_XX警报","B40167","AL[166]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[167]_单元6_XX警报","B40168","AL[167]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[168]_单元6_XX警报","B40169","AL[168]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[169]_单元6_XX警报","B40170","AL[169]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[170]_单元6_XX警报","B40171","AL[170]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[171]_单元6_XX警报","B40172","AL[171]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[172]_单元6_XX警报","B40173","AL[172]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[173]_单元6_XX警报","B40174","AL[173]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[174]_单元6_XX警报","B40175","AL[174]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[175]_单元6_XX警报","B40176","AL[175]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[176]_单元6_XX警报","B40177","AL[176]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[177]_单元6_XX警报","B40178","AL[177]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[178]_单元6_XX警报","B40179","AL[178]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[179]_单元6_XX警报","B40180","AL[179]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[180]_单元6_XX警报","B40181","AL[180]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[181]_单元6_XX警报","B40182","AL[181]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[182]_单元6_XX警报","B40183","AL[182]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[183]_单元6_XX警报","B40184","AL[183]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[184]_单元6_XX警报","B40185","AL[184]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[185]_单元6_XX警报","B40186","AL[185]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[186]_单元6_XX警报","B40187","AL[186]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[187]_单元6_XX警报","B40188","AL[187]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[188]_单元6_XX警报","B40189","AL[188]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[189]_单元6_XX警报","B40190","AL[189]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[190]_单元6_XX警报","B40191","AL[190]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","作业模块\n line_module","AL[191]_单元6_XX警报","B40192","AL[191]_单元6_XX警报","故障类型：警报alarm","fault_codes[6].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[192]_工位7_XX报警","B40193","AL[192]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[193]_工位7_XX报警","B40194","AL[193]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[194]_工位7_XX报警","B40195","AL[194]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[195]_工位7_XX报警","B40196","AL[195]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[196]_工位7_XX报警","B40197","AL[196]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[197]_工位7_XX报警","B40198","AL[197]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[198]_工位7_XX报警","B40199","AL[198]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[199]_工位7_XX报警","B40200","AL[199]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[200]_工位7_XX报警","B40201","AL[200]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[201]_工位7_XX报警","B40202","AL[201]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[202]_工位7_XX报警","B40203","AL[202]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[203]_工位7_XX报警","B40204","AL[203]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[204]_工位7_XX报警","B40205","AL[204]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[205]_工位7_XX报警","B40206","AL[205]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[206]_工位7_XX报警","B40207","AL[206]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[207]_工位7_XX报警","B40208","AL[207]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[208]_工位7_XX报警","B40209","AL[208]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[209]_工位7_XX报警","B40210","AL[209]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[210]_工位7_XX报警","B40211","AL[210]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[211]_工位7_XX报警","B40212","AL[211]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[212]_工位7_XX报警","B40213","AL[212]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[213]_工位7_XX报警","B40214","AL[213]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[214]_工位7_XX报警","B40215","AL[214]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[215]_工位7_XX报警","B40216","AL[215]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[216]_工位7_XX报警","B40217","AL[216]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[217]_工位7_XX报警","B40218","AL[217]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[218]_工位7_XX报警","B40219","AL[218]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[219]_工位7_XX报警","B40220","AL[219]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[220]_工位7_XX报警","B40221","AL[220]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[221]_工位7_XX报警","B40222","AL[221]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[222]_工位7_XX报警","B40223","AL[222]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[223]_工位7_XX报警","B40224","AL[223]_工位7_XX报警","故障类型：警报alarm","fault_codes[7].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[224]_工位8_XX报警","B40225","AL[224]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[225]_工位8_XX报警","B40226","AL[225]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[226]_工位8_XX报警","B40227","AL[226]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[227]_工位8_XX报警","B40228","AL[227]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[228]_工位8_XX报警","B40229","AL[228]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[229]_工位8_XX报警","B40230","AL[229]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[230]_工位8_XX报警","B40231","AL[230]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[231]_工位8_XX报警","B40232","AL[231]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[232]_工位8_XX报警","B40233","AL[232]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[233]_工位8_XX报警","B40234","AL[233]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[234]_工位8_XX报警","B40235","AL[234]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[235]_工位8_XX报警","B40236","AL[235]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[236]_工位8_XX报警","B40237","AL[236]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[237]_工位8_XX报警","B40238","AL[237]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[238]_工位8_XX报警","B40239","AL[238]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[239]_工位8_XX报警","B40240","AL[239]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[240]_工位8_XX报警","B40241","AL[240]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[241]_工位8_XX报警","B40242","AL[241]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[242]_工位8_XX报警","B40243","AL[242]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[243]_工位8_XX报警","B40244","AL[243]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[244]_工位8_XX报警","B40245","AL[244]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[245]_工位8_XX报警","B40246","AL[245]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[246]_工位8_XX报警","B40247","AL[246]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[247]_工位8_XX报警","B40248","AL[247]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[248]_工位8_XX报警","B40249","AL[248]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[249]_工位8_XX报警","B40250","AL[249]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[250]_工位8_XX报警","B40251","AL[250]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[251]_工位8_XX报警","B40252","AL[251]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[252]_工位8_XX报警","B40253","AL[252]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[253]_工位8_XX报警","B40254","AL[253]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[254]_工位8_XX报警","B40255","AL[254]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[255]_工位8_XX报警","B40256","AL[255]_工位8_XX报警","故障类型：警报alarm","fault_codes[8].31","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[256]_工位9_XX报警","B40257","AL[256]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].0","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[257]_工位9_XX报警","B40258","AL[257]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].1","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[258]_工位9_XX报警","B40259","AL[258]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].2","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[259]_工位9_XX报警","B40260","AL[259]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].3","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[260]_工位9_XX报警","B40261","AL[260]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].4","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[261]_工位9_XX报警","B40262","AL[261]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].5","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[262]_工位9_XX报警","B40263","AL[262]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].6","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[263]_工位9_XX报警","B40264","AL[263]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].7","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[264]_工位9_XX报警","B40265","AL[264]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].8","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[265]_工位9_XX报警","B40266","AL[265]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].9","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[266]_工位9_XX报警","B40267","AL[266]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].10","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[267]_工位9_XX报警","B40268","AL[267]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].11","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[268]_工位9_XX报警","B40269","AL[268]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].12","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[269]_工位9_XX报警","B40270","AL[269]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].13","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[270]_工位9_XX报警","B40271","AL[270]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].14","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[271]_工位9_XX报警","B40272","AL[271]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].15","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[272]_工位9_XX报警","B40273","AL[272]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].16","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[273]_工位9_XX报警","B40274","AL[273]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].17","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[274]_工位9_XX报警","B40275","AL[274]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].18","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[275]_工位9_XX报警","B40276","AL[275]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].19","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[276]_工位9_XX报警","B40277","AL[276]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].20","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[277]_工位9_XX报警","B40278","AL[277]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].21","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[278]_工位9_XX报警","B40279","AL[278]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].22","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[279]_工位9_XX报警","B40280","AL[279]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].23","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[280]_工位9_XX报警","B40281","AL[280]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].24","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[281]_工位9_XX报警","B40282","AL[281]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].25","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[282]_工位9_XX报警","B40283","AL[282]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].26","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[283]_工位9_XX报警","B40284","AL[283]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].27","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[284]_工位9_XX报警","B40285","AL[284]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].28","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[285]_工位9_XX报警","B40286","AL[285]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].29","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[286]_工位9_XX报警","B40287","AL[286]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].30","左工位"]
["胶线检测","C-PFA-CPAIGL-A-BZJG-0001","故障日志\n fault_log","电气控制\nelectric_control","警报\nalarm","流水线模块\n line_module","AL[287]_工位9_XX报警","B40288","AL[287]_工位9_XX报警","故障类型：警报alarm","fault_codes[9].31","左工位"]